/*
*
* Copyright (c) 2021 Darryl deHaan
* SPDX-License-Identifier: MIT
*
*/

/dts-v1/;
#include <nordic/nrf52840_qiaa.dtsi>

#include <dt-bindings/zmk/matrix_transform.h>

/ {
    model = "Corne-ish Zen";
    compatible = "corneish_zen";

    chosen {
        zephyr,code-partition = &code_partition;
        zephyr,sram = &sram0;
        zephyr,flash = &flash0;
        zmk,kscan = &kscan0;
        zmk,display = &epd;
        zephyr,console = &cdc_acm_uart;
        zmk,matrix_transform = &default_transform;
    };

    default_transform: keymap_transform_0 {
        compatible = "zmk,matrix-transform";
        columns = <12>;
        rows = <4>;

            // | SW1  | SW2  | SW3  | SW4  | SW5  | SW6  |   | SW6  | SW5  | SW4  | SW3  | SW2  | SW1  |
            // | SW7  | SW8  | SW9  | SW10 | SW11 | SW12 |   | SW12 | SW11 | SW10 | SW9  | SW8  | SW7  |
            // | SW13 | SW14 | SW15 | SW16 | SW17 | SW18 |   | SW18 | SW17 | SW16 | SW15 | SW14 | SW13 |
            //                      | SW19 | SW20 | SW21 |   | SW21 | SW20 | SW19 |
                    map = <
            RC(0,0) RC(0,1) RC(0,2) RC(0,3) RC(0,4) RC(0,5)  RC(0,6) RC(0,7) RC(0,8) RC(0,9) RC(0,10) RC(0,11)
            RC(1,0) RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(1,5)  RC(1,6) RC(1,7) RC(1,8) RC(1,9) RC(1,10) RC(1,11)
            RC(2,0) RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(2,5)  RC(2,6) RC(2,7) RC(2,8) RC(2,9) RC(2,10) RC(2,11)
                                    RC(3,3) RC(3,4) RC(3,5)  RC(3,6) RC(3,7) RC(3,8)
        >;
    };

    five_column_transform: keymap_transform_1 {
        compatible = "zmk,matrix-transform";
        columns = <10>;
        rows = <4>;

            // | SW2  | SW3  | SW4  | SW5  | SW6  |   | SW6  | SW5  | SW4  | SW3  | SW2  |
            // | SW8  | SW9  | SW10 | SW11 | SW12 |   | SW12 | SW11 | SW10 | SW9  | SW8  |
            // | SW14 | SW15 | SW16 | SW17 | SW18 |   | SW18 | SW17 | SW16 | SW15 | SW14 |
            //               | SW19 | SW20 | SW21 |   | SW21 | SW20 | SW19 |
        map = <
            RC(0,1) RC(0,2) RC(0,3) RC(0,4) RC(0,5)  RC(0,6) RC(0,7) RC(0,8) RC(0,9) RC(0,10)
            RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(1,5)  RC(1,6) RC(1,7) RC(1,8) RC(1,9) RC(1,10)
            RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(2,5)  RC(2,6) RC(2,7) RC(2,8) RC(2,9) RC(2,10)
                            RC(3,3) RC(3,4) RC(3,5)  RC(3,6) RC(3,7) RC(3,8)
        >;
    };

};

&adc {
    status = "okay";
};

&gpiote {
    status = "okay";
};

&gpio0 {
    status = "okay";
};

&gpio1 {
    status = "okay";
};

&usbd {
    status = "okay";
    cdc_acm_uart: cdc_acm_uart {
        compatible = "zephyr,cdc-acm-uart";
        label = "CDC_ACM_0";
    };
};

&flash0 {
    /*
     * For more information, see:
     * http://docs.zephyrproject.org/latest/devices/dts/flash_partitions.html
     */
    partitions {
        compatible = "fixed-partitions";
        #address-cells = <1>;
        #size-cells = <1>;

        sd_partition: partition@0 {
            label = "softdevice";
            reg = <0x00000000 0x00026000>;
        };
        code_partition: partition@26000 {
            label = "code_partition";
            reg = <0x00026000 0x000c6000>;
        };

        /*
         * The flash starting at 0x000ec000 and ending at
         * 0x000f3fff is reserved for use by the application.
         */

        /*
         * Storage partition will be used by FCB/LittleFS/NVS
         * if enabled.
         */
        storage_partition: partition@ec000 {
            label = "storage";
            reg = <0x000ec000 0x00008000>;
        };

        boot_partition: partition@f4000 {
            label = "adafruit_boot";
            reg = <0x000f4000 0x0000c000>;
        };
    };
};
